**Section D101**

**General**

**D102.1 Access and loading**. Facilities, buildings or portions of buildings hereafter constructed shall be accessible to fire department apparatus by way of an approved fire apparatus access road with an asphalt, concrete or other approved driving surface cable of supporting the imposed load of fire apparatus weighing up to 85,000 pounds (38,555kg).